;
;  Purpose:   Netcard setup information file for Windows 7
;
;  Author:    Anders Ma
;
;  Date:      August, 2010
;
;  Copyright: VIA Technologies, Inc.
;

[Version]
CatalogFile = netvfx64.cat
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Prov%
Compatible  = 1
DriverVer   = 08/06/2010, 1.13.0.2

[Manufacturer]
%Manuf%     = MANUF, NTAMD64

[ControlFlags]
ExcludeFromSelect = *

[MANUF.NTAMD64]
%GEN106S.DeviceDesc%    = VT3106S.ndi, PCI\VEN_1106&DEV_3053
%GEN106J.DeviceDesc%    = VT3106J.ndi, PCI\VEN_1106&DEV_3106
%GEN65.DeviceDesc%      = VT3065.ndi,  PCI\VEN_1106&DEV_3065
%GEN43.DeviceDesc%      = VT3043.ndi,  PCI\VEN_1106&DEV_3043
%VT3106S.DeviceDesc%    = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_01061106
%VT3106J.DeviceDesc%    = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_01051106
%VT3065.DeviceDesc%     = VT3065.ndi,  PCI\VEN_1106&DEV_3065&SUBSYS_01021106
%VT3043.DeviceDesc%     = VT3043.ndi,  PCI\VEN_1106&DEV_3043&SUBSYS_01001106
%VT3043.DeviceDesc%     = VT3043.ndi,  PCI\VEN_1106&DEV_3043&SUBSYS_0100086C

;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_02001014
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_029014CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_466014CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_466A14CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_800114CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_700114CD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_700914CD
;(27)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70681071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_71701071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_73681071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_01241071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_85561071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_83751071
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_80821071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_01031071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_83991071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_88891071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_104113BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_104413BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_102213BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_102413BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_104713BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_104B13BD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0081631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0091631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0151631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0271631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_86661071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_89651071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_86501071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_86551071
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10AB1734
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10B31734
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_85151071
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A70110FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A70010FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A71510FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A71610FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A71710FD
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A80010FD
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81001584
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81101584
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81201584
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10321734
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E00E1631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_81321584
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_15031043
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_80C71043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80FF1043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80A11043
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80ED1043
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_20061B0A
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_101E1025
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_003E1025
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B710156D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B7261019
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_3185109F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7143109F
;(28)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90011509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_901F1509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90201509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90211509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90221509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90231509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90241509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90251509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90261509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90271509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90281509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_28201509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90481509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92121509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_905F1509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92161509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_35301509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_90561509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92201509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92211509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92321509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92331509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92341509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92351509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92361509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_92571509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1D411509
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1E201509
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10F71734
;(18)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0077A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0088A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00C3A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00C7A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_016FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_042FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_041DA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_042FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0439A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_046FA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_044BA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_043AA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_04CFA0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_04D1A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_04D2A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0613A0A0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0617A0A0
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_0702A0A0
;(5)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70021631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_D0021631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_D0031631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E0101631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E0281631
;(3)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10291025
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_006E1025
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_108F17C0
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0028103C
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E0001458
;(9)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_900B1695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30031695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30051695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30041695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30061695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_217614A4
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_300C1695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_300D1695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_300E1695
;(51)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A2321297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8001297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8011297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8021297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8031297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8041297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8051297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8061297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8071297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8081297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8091297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80A1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80B1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80C1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80D1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80E1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C80F1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8101297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8111297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8121297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8131297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8141297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8151297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8161297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8171297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8181297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8191297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81A1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81B1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81C1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81D1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81E1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C81F1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8201297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8211297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8221297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8231297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8241297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8251297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8261297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8271297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8281297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C8291297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82A1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82B1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82C1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82D1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82E1297
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C82F1297
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_51701297
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_31701297
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_15D40015
;(17)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_2718270F
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_271B270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7552270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7553270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7576270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7577270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7578270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7649270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7660270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7664270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7668270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7669270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7178270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7840270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_FC10270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7671270F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_7672270F
;(3)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1400147B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1401147B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1402147B
;(95)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A781019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A791019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A801019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A811019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A821019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A831019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A841019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A851019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A861019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18311019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18321019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18331019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18341019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18351019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18361019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18371019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18381019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18391019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18401019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18411019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18421019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18431019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18441019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18451019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18461019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18471019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18481019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18491019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18501019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18511019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18521019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18531019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18541019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18551019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18561019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18571019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18581019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18591019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18601019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A361019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A691019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A711019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A721019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A731019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A741019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A751019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A761019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0A771019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F101019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B7261019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B3201019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F251019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18921019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18931019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18941019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18951019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18961019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18971019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18981019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_18991019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70331019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B411019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B421019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B431019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B441019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B451019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B461019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B471019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B481019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B491019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B501019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B511019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B521019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B531019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B541019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B551019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B561019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B571019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B581019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B591019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B601019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B611019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B621019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B631019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B641019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B651019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B661019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B671019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B681019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B691019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_1B701019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F601019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_01021019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F751019
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0F791019
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00011843
;(9)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10011816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10021816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10041816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_10051816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_40011816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_40021816
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_30011816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20021816
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20011816
;(4)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5150107D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5151107D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5130107D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_5135107D
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_233310F1
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_249010F1
;(28)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_60101106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_60151106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_60171106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0031106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0041106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0061106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0071106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0081106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A0091106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_B0031106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_B0051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B0061106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B0071106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B0081106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0021106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0031106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_C0051106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_C0061106
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_C0071106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0081106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA011106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA021106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA031106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_AA041106
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_AA051106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_CC011106
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_CC021106
;(32)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_390C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_593C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_596C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_712C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_716C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_707C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_72301462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_723C1462
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_747C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_762C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_768C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_775C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_778C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_015C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_014C1462
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_012C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_750C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C01C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C02C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C03C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C04C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_021C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70951462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_075C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_70611462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_016C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_74101462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_787C1462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_72931462
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_902E1695
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E0281631
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_10001462
;(4)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_140217F2
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_140617F2
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_140717F2
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_140B17F2
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_30431849
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_923017C4
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_8000105B
;(3)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_217514A4
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_218214A4
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_217614A4
;(13)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_040814FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_020C14FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_020D14FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_020E14FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_021314FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_021414FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A00214FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A00714FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A00F14FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A01114FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A01214FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_A01414FF
%VT3106S.DeviceDesc% = VT3106S.ndi, PCI\VEN_1106&DEV_3053&SUBSYS_A02314FF
;(5)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_202B161F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_2032161F
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_2033161F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_2037161F
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0216107B
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_001214C0
;(13)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_200A1558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_05701558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_54021558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_06621558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_54061558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_54081558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_06631558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_06641558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_06651558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_80011558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_54091558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_06681558
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_06691558
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00331025
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0713152D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0760152D
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_C0181631
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_FF311179
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_FF101179
;(5)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00011170
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_00021170
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_000817FF
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10D91734
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_10D91170
;(2)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_010216F3
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_010516F3
;(16)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120018D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120118D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120218D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120318D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120418D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120518D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120618D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120718D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120818D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120918D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120A18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120B18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120C18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120D18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120E18D0
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_120F18D0
;(16)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C12105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C13105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C14105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C15105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C16105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C17105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C18105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C19105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C1A105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C1B105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C1C105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C1D105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C1E105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0C1F105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0CF1105B
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_0CD8105B
;(1)
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_00031FC2
;(5)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20011919
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20021919
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20031919
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20041919
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_20061919
;(6)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_61131915
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_61001915
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_61011915
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_61021915
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_61031915
%VT3106J.DeviceDesc% = VT3106J.ndi, PCI\VEN_1106&DEV_3106&SUBSYS_61041915
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_E0001940
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B3001897
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_B02D144D
;(1)
%VT3065.DeviceDesc% = VT3065.ndi,   PCI\VEN_1106&DEV_3065&SUBSYS_100817AA

;-------------------------------------------------------------------------------
; ndi for 3106S
;-------------------------------------------------------------------------------
[VT3106S.ndi.NTAMD64]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg, FET.SW.delreg
AddReg          = VT3106S.reg, FET.reg, FlowCtrl.reg, AI.reg, Wakeup.reg, pQ.reg, ChecksumOffload.reg, FET.SW.NT
CopyFiles       = FET.CopyFiles.NTAMD64, FET.SW.CopyFiles.NTAMD64
*IfType            = 6 ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0 ; NdisMedium802_3
*PhysicalMediaType = 0 ; NdisPhysicalMediumUnspecified

[VT3106S.ndi.NTAMD64.Services]
AddService      = FETNDIS, 2, FET_NTAMD64.Service, FET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3106J
;-------------------------------------------------------------------------------
[VT3106J.ndi.NTAMD64]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg, FET.SW.delreg
AddReg          = VT3106J.reg, FET.reg, FlowCtrl.reg, AI.reg, Wakeup.reg, FET.SW.NT
CopyFiles       = FET.CopyFiles.NTAMD64, FET.SW.CopyFiles.NTAMD64
*IfType            = 6 ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0 ; NdisMedium802_3
*PhysicalMediaType = 0 ; NdisPhysicalMediumUnspecified

[VT3106J.ndi.NTAMD64.Services]
AddService      = FETNDIS, 2, FET_NTAMD64.Service, FET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3065
;-------------------------------------------------------------------------------
[VT3065.ndi.NTAMD64]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg, FET.SW.delreg
AddReg          = VT3065.reg, FET.reg, FlowCtrl.reg, AI.reg, Wakeup.reg, FET.SW.NT
CopyFiles       = FET.CopyFiles.NTAMD64, FET.SW.CopyFiles.NTAMD64
*IfType            = 6 ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0 ; NdisMedium802_3
*PhysicalMediaType = 0 ; NdisPhysicalMediumUnspecified

[VT3065.ndi.NTAMD64.Services]
AddService      = FETNDIS, 2, FET_NTAMD64.Service, FET.EventLog

;-------------------------------------------------------------------------------
; ndi for 3043
;-------------------------------------------------------------------------------
[VT3043.ndi.NTAMD64]
Characteristics = 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         = 5
DelReg          = FET.delreg, FET.SW.delreg
AddReg          = VT3043.reg, FET.reg, FET.SW.NT
CopyFiles       = FET.CopyFiles.NTAMD64, FET.SW.CopyFiles.NTAMD64
*IfType            = 6 ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0 ; NdisMedium802_3
*PhysicalMediaType = 0 ; NdisPhysicalMediumUnspecified

[VT3043.ndi.NTAMD64.Services]
AddService      = FETNDIS, 2, FET_NTAMD64.Service, FET.EventLog


;-------------------------------------------------------------------------------
; VT3106S specific
;
[VT3106S.reg]
HKR, Ndi,                           DeviceID,   0, "PCI\VEN_1106&DEV_3053"

;-------------------------------------------------------------------------------
; VT3106J specific
;
[VT3106J.reg]
HKR, Ndi,                           DeviceID,   0, "PCI\VEN_1106&DEV_3106"

;-------------------------------------------------------------------------------
; VT3065 specific
;
[VT3065.reg]
HKR, Ndi,                           DeviceID,   0, "PCI\VEN_1106&DEV_3065"

;-------------------------------------------------------------------------------
; VT3043 specific
;
[VT3043.reg]
HKR, Ndi,                           DeviceID,   0, "PCI\VEN_1106&DEV_3043"


;-------------------------------------------------------------------------------
; FET common driver parameters
;
[FET.reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "FETNDIS"

HKR, ,                                      ReceiveBurstIndicate, 0,"64"
HKR, ,                                      ReceiveThreshold,     0, "0"
HKR, ,                                      TransmitThreshold,    0, "0"
HKR, ,                                      BurstLength,          0, "1"

; Nway Forced Mode
HKR, ,                                      NwayForce,            0, "1"

; Power Management Capability
HKR, ,                                      PMC,                  0, "0"

; Validate Rx SNAP/802.3 packet length
HKR, ,                                      ValidatePacketLen,    0, "0"

; User defined Network Address (standardized keyword)
HKR, ,                                      NetworkAddress,       0, ""
HKR, Ndi\params\NetworkAddress,             ParamDesc,            0, %NetAddress%
HKR, Ndi\params\NetworkAddress,             Default,              0, ""
HKR, Ndi\params\NetworkAddress,             type,                 0, "edit"
HKR, NDI\params\NetworkAddress,             LimitText,            0, "12"
HKR, NDI\params\NetworkAddress,             UpperCase,            0, "1"
HKR, NDI\params\NetworkAddress,             optional,             0, "1"
HKR, NDI\params\NetworkAddress,             Base,                 0, "16"

; Tx Buffers (standardized keyword)
HKR, ,                                      *TransmitBuffers,     0, "160"
HKR, Ndi\params\*TransmitBuffers,           ParamDesc,            0, %TXBuffer%
HKR, Ndi\params\*TransmitBuffers,           default,              0, "160"
HKR, Ndi\params\*TransmitBuffers,           type,                 0, "int"
HKR, Ndi\params\*TransmitBuffers,           Min,                  0, "64"
HKR, Ndi\params\*TransmitBuffers,           Max,                  0, "256"
HKR, Ndi\params\*TransmitBuffers,           Step,                 0, "1"
HKR, Ndi\params\*TransmitBuffers,           Base,                 0, "10"

; Rx Buffers (standardized keyword)
HKR, ,                                      *ReceiveBuffers,      0, "160"
HKR, Ndi\params\*ReceiveBuffers,            ParamDesc,            0, %RXBuffer%
HKR, Ndi\params\*ReceiveBuffers,            default,              0, "160"
HKR, Ndi\params\*ReceiveBuffers,            type,                 0, "int"
HKR, Ndi\params\*ReceiveBuffers,            Min,                  0, "64"
HKR, Ndi\params\*ReceiveBuffers,            Max,                  0, "256"
HKR, Ndi\params\*ReceiveBuffers,            Step,                 0, "1"
HKR, Ndi\params\*ReceiveBuffers,            Base,                 0, "10"

; Connection Type (standardized keyword)
HKR, ,                                      *SpeedDuplex,         0, "0"
HKR, Ndi\params\*SpeedDuplex,               ParamDesc,            0, %SpeedDuplexSet%
HKR, Ndi\params\*SpeedDuplex,               default,              0, "0"
HKR, Ndi\params\*SpeedDuplex,               type,                 0, "enum"
HKR, Ndi\params\*SpeedDuplex\enum,          "0",                  0, %autoN%
HKR, Ndi\params\*SpeedDuplex\enum,          "1",                  0, %10HD%
HKR, Ndi\params\*SpeedDuplex\enum,          "2",                  0, %10FD%
HKR, Ndi\params\*SpeedDuplex\enum,          "3",                  0, %100HD%
HKR, Ndi\params\*SpeedDuplex\enum,          "4",                  0, %100FD%

[FlowCtrl.reg]
; Flow control capability advertisement (standardized keyword)
HKR, ,                                      *FlowControl,         0, "0"
HKR, Ndi\params\*FlowControl,               ParamDesc,            0, %FlowCtl%
HKR, Ndi\params\*FlowControl,               default,              0, "0"
HKR, Ndi\params\*FlowControl,               type,                 0, "enum"
HKR, Ndi\params\*FlowControl\enum,          "0",                  0, %Disabled%
HKR, Ndi\params\*FlowControl\enum,          "3",                  0, %EnableRxTx%

[AI.reg]
; Interrupt Moderation (standardized keyword)
HKR, ,                                      *InterruptModeration, 0, "1"
HKR, Ndi\params\*InterruptModeration,       ParamDesc,            0, %AI%
HKR, Ndi\params\*InterruptModeration,       default,              0, "1"
HKR, Ndi\params\*InterruptModeration,       type,                 0, "enum"
HKR, Ndi\params\*InterruptModeration\enum,  "0",                  0, %Disabled%
HKR, Ndi\params\*InterruptModeration\enum,  "1",                  0, %Enabled%

[pQ.reg]
; number of Tx queue allocation
HKR, ,                                      TxQueueNum,           0, "8"

; 802.1p/802.1Q Packet Tagging (standardized keyword)
HKR, ,                                      *PriorityVLANTag,     0, "0"
HKR, Ndi\Params\*PriorityVLANTag,           ParamDesc,            0, %8021pq%
HKR, Ndi\Params\*PriorityVLANTag,           Default,              0, "0"
HKR, Ndi\Params\*PriorityVLANTag,           type,                 0, "enum"
HKR, Ndi\Params\*PriorityVLANTag\enum,      "0",                  0, %PQDisabled%
HKR, Ndi\Params\*PriorityVLANTag\enum,      "3",                  0, %PQEnabled%

; static single VLAN ID setting
HKR, ,                                      VLANID,               0, "0"
HKR, Ndi\params\VLANID,                     ParamDesc,            0, %VLANID%
HKR, Ndi\params\VLANID,                     default,              0, "0"
HKR, Ndi\params\VLANID,                     type,                 0, "int"
HKR, Ndi\params\VLANID,                     Min,                  0, "0"
HKR, Ndi\params\VLANID,                     Max,                  0, "4094"
HKR, Ndi\params\VLANID,                     Step,                 0, "1"
HKR, Ndi\params\VLANID,                     Base,                 0, "10"

[ChecksumOffload.reg]
; IPv4 IP Checksum (standardized keyword)
HKR, ,                                          *IPChecksumOffloadIPv4,   0, "3"
HKR, Ndi\params\*IPChecksumOffloadIPv4,         ParamDesc,                0, %IPCKSMv4%
HKR, Ndi\params\*IPChecksumOffloadIPv4,         default,                  0, "3"
HKR, Ndi\params\*IPChecksumOffloadIPv4,         type,                     0, "enum"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,    "0",                      0, %Disabled%
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,    "1",                      0, %EnableTx%
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,    "2",                      0, %EnableRx%
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,    "3",                      0, %EnableRxTx%

; IPv4 TCP Checksum (standardized keyword)
HKR, ,                                          *TCPChecksumOffloadIPv4,  0, "3"
HKR, Ndi\params\*TCPChecksumOffloadIPv4,        ParamDesc,                0, %TCPCKSMv4%
HKR, Ndi\params\*TCPChecksumOffloadIPv4,        default,                  0, "3"
HKR, Ndi\params\*TCPChecksumOffloadIPv4,        type,                     0, "enum"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,   "0",                      0, %Disabled%
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,   "1",                      0, %EnableTx%
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,   "2",                      0, %EnableRx%
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,   "3",                      0, %EnableRxTx%

; IPv4 UDP Checksum (standardized keyword)
HKR, ,                                          *UDPChecksumOffloadIPv4,  0, "3"
HKR, Ndi\params\*UDPChecksumOffloadIPv4,        ParamDesc,                0, %UDPCKSMv4%
HKR, Ndi\params\*UDPChecksumOffloadIPv4,        default,                  0, "3"
HKR, Ndi\params\*UDPChecksumOffloadIPv4,        type,                     0, "enum"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,   "0",                      0, %Disabled%
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,   "1",                      0, %EnableTx%
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,   "2",                      0, %EnableRx%
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,   "3",                      0, %EnableRxTx%

[Wakeup.reg]
; Wake on pattern match (standardized keyword) [NDIS 6.2]
HKR, ,                                          *WakeOnPattern,           0, "1"
HKR, Ndi\params\*WakeOnPattern,                 ParamDesc,                0, %WOPDesc%
HKR, Ndi\params\*WakeOnPattern,                 default,                  0, "1"
HKR, Ndi\params\*WakeOnPattern,                 type,                     0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,            "0",                      0, %Disabled%
HKR, Ndi\params\*WakeOnPattern\enum,            "1",                      0, %Enabled%

; Wake on Magic Packet (standardized keyword) [NDIS 6.2]
HKR, ,                                          *WakeOnMagicPacket,       0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,             ParamDesc,                0, %WOMDesc%
HKR, Ndi\params\*WakeOnMagicPacket,             default,                  0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,             type,                     0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,        "0",                      0, %Disabled%
HKR, Ndi\params\*WakeOnMagicPacket\enum,        "1",                      0, %Enabled%

;-------------------------------------------------------------------------------
; 64-bit uninstaller
[FET.SW.NT]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, Contact, 0, "http://www.via.com.tw/en/support/contact_us/"
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, DisplayName, 0, %Rhine.DeviceDesc%
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, HelpLink, 0, "http://www.via.com.tw/en/index.jsp"
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, Publisher, 0, %Manuf%
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, UninstallString, 0, "Rundll32.exe vuins64.dll,vuins64Ex $Rhine $VIA"
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, URLInfoAbout, 0, "http://www.via.com.tw/en/products/networking/"
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA, URLUpdateInfo, 0, "http://www.via.com.tw/en/support/drivers.jsp"
HKLM, Software\VN_VUIns\Rhine\VIA\DeviceIdList, 3065, 0, "0"
HKLM, Software\VN_VUIns\Rhine\VIA\DeviceIdList, 3053, 0, "0"
HKLM, Software\VN_VUIns\Rhine\VIA\DeviceIdList, 3106, 0, "0"
HKLM, Software\VN_VUIns\Rhine\VIA\DeviceIdList, 3043, 0, "0"

;-------------------------------------------------------------------------------
; Installation for NT
;

[FET.CopyFiles.NTAMD64]
fetn62a.sys,,,2

[FET.SW.CopyFiles.NTAMD64]
vuins64.dll,,,2
difxapi.dll,,,2

[FET_NTAMD64.Service]
DisplayName     = %FET.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\fetn62a.sys
LoadOrderGroup  = NDIS

[FET.EventLog]
AddReg = FET.AddEventLog.reg

[FET.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir            = 11
FET.CopyFiles.NTAMD64     = 12
FET.SW.CopyFiles.NTAMD64  = 11

[SourceDisksNames]
1 = %DiskName%,,

[SourceDisksFiles]
fetn62a.sys  = 1
vuins64.dll  = 1
difxapi.dll  = 1

;-------------------------------------------------------------------------------
; Uninstall/DelFiles/DelReg
;
[FET.delreg]
HKR,Ndi\Params

[FET.SW.delreg]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_Rhine_VIA
HKLM, Software\VN_VUIns\Rhine\VIA

;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
Prov                = "VIA"
DiskName            = "VIA Rhine Family Fast Ethernet Adapter driver disk"

SpeedDuplexSet      = "Speed & Duplex Settings"
autoN               = "Auto Negotiation"
10HD                = "10 Mbps Half Duplex"
10FD                = "10 Mbps Full Duplex"
100HD               = "100 Mbps Half Duplex"
100FD               = "100 Mbps Full Duplex"
RXBuffer            = "Receive Buffers"
TXBuffer            = "Transmit Buffers"
FlowCtl             = "Flow Control"
Disabled            = "Disabled"
Enabled             = "Enabled"
EnableTx            = "Tx enabled"
EnableRx            = "Rx enabled"
EnableRxTx          = "Rx & Tx enabled"
8021pq              = "Priority & VLAN"
PQDisabled          = "Priority & VLAN Disabled"
PQEnabled           = "Priority & VLAN Enabled"
AI                  = "InterruptModeration"
NetAddress          = "Network Address"
IPCKSMv4            = "IPv4 Checksum Offload"
TCPCKSMv4           = "TCP Checksum Offload (IPv4)"
UDPCKSMv4           = "UDP Checksum Offload (IPv4)"
WOPDesc             = "Wake on Pattern Match"
WOMDesc             = "Wake on Magic Packet"
VLANID              = "VLAN ID"
Wakeup              = "Wake up Type"
OSControl           = "OS Controlled"
Magic               = "Magic Packet"
Pattern             = "Pattern Match"
All                 = "ALL"

Manuf   = "VIA Technologies, Inc."
GEN106S.DeviceDesc    = "VIA Rhine III Compatible Management Adapter"
GEN106J.DeviceDesc    = "VIA Rhine III Compatible Fast Ethernet Adapter"
GEN65.DeviceDesc      = "VIA Rhine II Compatible Fast Ethernet Adapter"
GEN43.DeviceDesc      = "VIA VT86C100A Rhine Compatible Fast Ethernet Adapter"
VT3106S.DeviceDesc    = "VIA Rhine III Management Adapter"
VT3106J.DeviceDesc    = "VIA Rhine III Fast Ethernet Adapter"
VT3065.DeviceDesc     = "VIA Rhine II Fast Ethernet Adapter"
VT3043.DeviceDesc     = "VIA VT86C100A Rhine Fast Ethernet Adapter"
FET.Service.DispName = "VIA Rhine Family Fast Ethernet Adapter Driver"
Rhine.DeviceDesc     = "VIA Rhine Family Fast Ethernet Adapter"
